--------------------------------------------------------------------
MD32x0/MD32x0i/MD36x0i SAS HDD Firmware Update - Release A09
--------------------------------------------------------------------

During the next scheduled maintenance window, please update the drive firmware to the latest level.

To update Physical Disk firmware through a MD3200/MD3200i/ enclosure using
Dell Modular Disk Storage Manager (MDSM) management application, please follow the steps below:

1) From MDSM, click the Support tab, then click the Download Firmware link.

2) From the Download firmware display, click the Download Physical Disk Firmware link.  And then 
click the Next button.

3) A dialog box lists the current physical disk firmware version in use. Click the Add button
to browse to the file that matches the model number you want to download. 

4) Select the file in the File Selection area and then click OK. Only the firmware images that are 
compatible with physical disks in the storage array can be selected, and will appear in the "Selected 
Packages" window.  If the file you selected is not valid or is incompatible with the physical disks
in the storage array, an error message appears. Click OK to close it, and select a compatible file.

5) Continue steps 3 & 4 until the complete list of packages to be downloaded is displayed.
   
6) Press Next.

7) A Confirm Download dialog box appears listing the current versions and the versions you selected
of physical disk firmware. Select individual drives to be updated, or for all drives in the list,
click the "Select All" box. Then select Finish.

8) Type "yes" to confirm the firmware download.

---------------------------------------------------------------------------------------------------
HDD firmware update for MD32x0/MD32x0i/MD36x0i/MD36x0f and expanded MD12x0 storage arrays, rev A09
---------------------------------------------------------------------------------------------------

Description:
The information below describes the HDD firmware available and the known enhancements or fixes.
The following drives will be updated with the HDD firmware included in rev A09:

**Indicates firmware that is NEW for A09 release

------------------------------
Initial SAS HDD Release Firmware
------------------------------ 
37.0 Hitachi Ultrastar C10K600        2.5" 10K     version N2B4
40.0 Seagate (ST*00MM0006)	      2.5" 10k	   version LS06**
42.0 WD Verdi			      3.5" 7.2K	   version D1R2**
---------------------------
SAS HDD Firmware Updates
---------------------------
1.0  Seagate (Savvio 15K.2)           2.5" 15K.2,  version HT66**
2.0  Seagate (Savvio 15K.2)           2.5" 15K.2,  version HTF6
3.0  Seagate (Savvio 10K.3)           2.5" 10K.3,  version FS66**
4.0  Seagate (Savvio 10K.3)           2.5" 10K.3,  version FSF9
5.0  Seagate (Constellation 7200.1)   2.5" 7.2K,   version DS66**
6.0  Seagate (Constellation 7200.1)   2.5" 7.2K,   version DSF4
7.0  Seagate (Cheetah 15K.7)          3.5" 15.7K,  version ES66
8.0  Seagate (Cheetah 15K.7)          3.5" 15.7K,  version ESF7 
9.0  Seagate (Cheetah NS 10K.2)       3.5" 10.2K,  version ER65
10.0 Seagate (Constellation ES)       3.5" 7.2K,   version KS6B**
11.0 Seagate (Savvio 10K.4)           2.5" 10K.4,  version FM0A**
12.0 Seagate (Savvio 10K.4)           2.5" 10K.4,  version FMF2
13.0 Fujitsu (MBD2 RC)                2.5" 10K,    version D80A
14.0 Fujitsu (MBE2 RC)                2.5" 15K,    version D906
15.0 Hitachi 10K RPM                  2.5" 10K,    version J516
16.0 Hitachi 15K RPM                  2.5" 15K,    version K516
17.0 Hitachi 15K RPM                  2.5" 15K,    version E516
19.0 Seagate (Constellation ES)       3.5" 7.2K,   version KSF2
20.0 Western Digital (SL200M)         2.5" 10K,    version D1VB**
21.0 Western Digital (SL500M)         3.5" 7.2K,   version D1BG**
22.0 Hitachi (Ultrastar C10K600)      2.5" 10K,    version A360
23.0 Seagate Constellation.2          2.5" 7.2K,   version AS06
24.0 Toshiba (MBF 2 RC) 10K RPM       2.5" 10K,    version DA07
25.0 Toshiba MK2001TRKB Series        3.5" 7.2K,   version DCAA
26.0 Seagate Savvio 10K.5             2.5" 10K.5   version CS08
27.0 Seagate (Constellation ES.2)     2.5" 7.2K,   version ASF9
28.0 Seagate (Constellation ES.2)     3.5" 7.2K,   version RSFA
29.0 Seagate (Savvio 10K.5)           2.5" 10K,    version CSF8
30.0 Seagate (Savvio 15K.3)           2.5" 15K,    version YSF9
31.0 Seagate (Savvio 15K.3)           2.5" 15K,    version YS09
32.0 Seagate (Constellation ES.2)     3.5" 7.2K,   version RS11
33.0 Seagate (Constellation ES)       3.5" 7.2K,   version PS07
35.0 Western Digital (SL300M)	      2.5" 10K	   version D1S4
36.0 Hitachi Ultrastar 7K3000         3.5" 7.2K    version M2D4
38.0 Toshiba AL12SX		      2.5" 15k,	   version DB05
39.0 Toshiba AL12SE		      2.5", 10k,   version DA0B   


---------------------------
SSD Firmware Updates
---------------------------
18.0  Pliant Lightning LB150          2.5"         version D012
34.0 Toshiba MD2001GRZB Series        2.5"         version A006
41.0 Sandisk Everest		      2.5"	   version D313**

-------------------------------------------------------------------------------------
1.0 Seagate (Savvio 15K.2) SAS 73GB 15K RPM 2.5", version HT66
-------------------------------------------------------------------------------------
Fixes / Enhancements:

Resolves a performance issue that can occur when running background scans
Resolves a rare issue that can cause drive to hang on power cycle
Resolves an issue with dual port configurations when receiving same command on both ports 
Improved drive connectivity
Improved error handling
Improved SMART error logging

Model #		     Criticality 	       File Name
---------------	------------------   ----------------------------
ST973452SS	     Recommended        Seagate_ST973452SS_HT66.df 
ST9146852SS          Recommended        Seagate_ST9146852SS_HT66.df


-------------------------------------------------------------------------------
2.0 Seagate (Savvio 15K.2)  2.5" 15K, version HTF6
-------------------------------------------------------------------------------
Fixes / Enchancements:

- Fixed issue when hard reset occurred on port other than which data transfer was taking place
- Improved error handling when Notify Power Loss Expected sequence is initiated
- Improved performance of write operations in extreme temperature environments.
- Improved drive error handling
- Improved long term reliability of drive.
- Improved performance related to SED commands  

Model #	           Criticality			File Name
---------------	------------------   --------------------------------
ST9146752SS        Recommended          Seagate_ST9146752SS_HTF6.df


----------------------------------------------------------------------------------
3.0 Seagate (Savvio 10K.3)  2.5" 15K, version FS66
----------------------------------------------------------------------------------
Fixes / Enhancements:

Resolves a performance issue that can occur when running background scans
Resolves a rare issue that can cause drive to hang on power cycle
Resolves an issue with dual port configurations when receiving same command on both ports 
Improved drive connectivity
Improved error handling
Improved SMART error logging  

Model #	           Criticality			File Name
---------------	------------------   ----------------------------
ST9146803SS        Recommended          Seagate_ST9146803SS_FS66.df
ST9300603SS        Recommended          Seagate_ST9300603SS_FS66.df


----------------------------------------------------------------------------------
4.0 Seagate (Savvio 10K.3)  2.5" 10K, version FSF9
----------------------------------------------------------------------------------
Fixes / Enchancements:

- Fixed issue when hard reset occurred on port other than which data transfer was taking place
- Improved error handling when Notify Power Loss Expected sequence is initiated
- Improved performance of write operations in extreme temperature environments.
- Improved drive error handling
- Improved long term reliability of drive.
- Improved performance related to SED commands  

Model #	           Criticality			File Name
---------------	------------------   ---------------------------------
ST9300503SS        Recommended          Seagate_ST9300503SS_FSF9.df


----------------------------------------------------------------------------------
5.0 Seagate (Constellation 7200.1) 2.5" 7.2K, version DS66
----------------------------------------------------------------------------------
Fixes / Enhancements:

Resolves a performance issue that can occur when running background scans
Resolves a rare issue that can cause drive to hang on power cycle
Resolves an issue with dual port configurations when receiving same command on both ports 
Improved drive connectivity
Improved error handling
Improved SMART error logging

Model #	           Criticality			File Name
---------------	------------------   ---------------------------------
ST9500430SS        Recommended          Seagate_ST9500430SS_DS66.df


----------------------------------------------------------------------------------
6.0 Seagate (Constellation 7200.1) 2.5" 7.2K, version DSF4
----------------------------------------------------------------------------------
Fixes / Enchancements:

- Fixed issue when hard reset occurred on port other than which data transfer was taking place
- Improved error handling when Notify Power Loss Expected sequence is initiated
- Improved performance of write operations in extreme temperature environments.
- Improved drive error handling
- Improved long term reliability of drive.
- Improved performance related to SED commands 

Model #	           Criticality			File Name
---------------	------------------   ---------------------------------
ST9500431SS        Recommended          Seagate_ST9500431SS_DSF4.df


---------------------------------------------------------------------------
7.0 Seagate (Cheetah 15K.7) 3.5" 15.7K, version ES66
---------------------------------------------------------------------------
Fixes / Enhancements:

-Resolved an issue that caused drive to connect at slower connection speeds
-Resolved an issue causing poor write performance when background scan is running
-Resolved rare issue that could cause hang during boot up with RAID controller
-Resolved issue would unexpectedly abort read command without proper reporting proper status
-Improvements to drive connectivity
-Improved drive error handling 

Model#          Criticality     File Name
-------------	-----------    ----------------------------
ST3300657SS     Recommended     Seagate_ST3300657SS_ES66.df
ST3450857SS     Recommended     Seagate_ST3450857SS_ES66.df
ST3600057SS     Recommended     Seagate_ST3600057SS_ES66.df


------------------------------------------------------------------------------
8.0 Seagate (Cheetah 15K.7) 3.5" 15.7K, version ESF7
------------------------------------------------------------------------------
Fixes and Enhancements:

-Resolved an issue that caused drive to connect at slower connection speeds
-Resolved an issue causing poor write performance when background scan is running
-Resolved rare issue that could cause hang during boot up with RAID controller
-Resolved issue would unexpectedly abort read command without proper reporting proper status
-Improvements to drive connectivity
-Improved drive error handling

Model #		      Criticality	   File Name
---------------	 --------------	  -----------------------------------
ST3450757SS       Recommended	   Seagate_ST3450757SS_ESF7_450.df
ST3600957SS       Recommended	   Seagate_ST3600957SS_ESF7_600.df


----------------------------------------------------------------------------------
9.0 Seagate (Cheetah NS 10K.2) 3.5" SAS 10K, version ER66
----------------------------------------------------------------------------------
Fixes and Enhancements:

Resolves a performance issue that can occur when running background scans
Resolves a rare issue that can cause drive to hang on power cycle
Resolves an issue with dual port configurations when receiving same command on both ports 
Improved drive connectivity
Improved error handling
Improved SMART error logging 

Model #	         Criticality			File Name
--------------  ---------------     -----------------------------
ST3600002SS      Recommended         Seagate_ST3600002SS_ER66.df


---------------------------------------------------------------------------------------
10.0 Seagate (Constellation ES) 3.5" SAS 7.2K, version KS6B
---------------------------------------------------------------------------------------
Fixes and Enhancements:

Resolves a performance issue that can occur when running background scans
Resolves a rare issue that can cause drive to hang on power cycle
Resolves an issue with dual port configurations when receiving same command on both ports 
Improved drive connectivity
Improved error handling
Improved SMART error logging

Model#              Criticality     File Name
---------------     -----------	  ----------------------------
ST3500414SS         Recommended   Seagate_ST3500414SS_KS6B.df 
ST31000424SS        Recommended   Seagate_ST31000424SS_KS6B.df 
ST32000444SS        Recommended   Seagate_ST32000444SS_KS6B.df 


--------------------------------------------------------------------------------
11.0 Seagate (Savvio 10K.4) 2.5" SAS 10K.4, version FM0A**
--------------------------------------------------------------------------------
Fixes / Enhancements:
Resolves a performance issue that can occur when running background scans
Resolves a rare issue that can cause drive to hang on power cycle
Resolves an issue with dual port configurations when receiving same command on both ports 
Improved drive connectivity
Improved error handling
Improved SMART error logging

Model#         Criticality   File Name
-------------  -----------   ---------------------------
ST9600204SS    Recommended   Seagate_ST9600204SS_FM0A.df


--------------------------------------------------------------------------------
12.0 Seagate (Savvio 10K.4) 2.5" SAS 10K, version FMF2
--------------------------------------------------------------------------------

Model #				 File Name
-------------------- ------------------------------------
ST9600104SS        Firmware version FMF2 (pre-load)


-----------------------------------------------------------------------
13.0 Fujitsu (MBD2 RC) SAS 10K, version D80A
-----------------------------------------------------------------------
Fixes / Enhancements:

Resolve non-critial issue with drive in iSCSI enclousure 

Model #	        Criticality	    File Name
-------------  -------------   ----------------------------
MBD2300RC       Recommended     Fujitsu_MBD2300RC_D80A.df
MBD2147RC       Recommended     Fujitsu_MBD2147RC_D80A.df


-----------------------------------------------------------------------
14.0 Fujitsu (MBE2 RC) SAS 15K, version D906
-----------------------------------------------------------------------
Fixes / Enhancements:

Resolve non-critial issue with drive in iSCSI enclousure   

Model#          Criticality     File Name
-------------  -------------   ---------------------------
MBE2073RC       Recommended     Fujitsu_MBE2073RC_D906.df
MBE2147RC       Recommended     Fujitsu_MBE2147RC_D906.df


-----------------------------------------------------------------------
15.0 Hitachi SAS 10K RPM, version J516
-----------------------------------------------------------------------
Fixes / Enhancments:

- Fixed rare timeout issue that can occur during a drive reset
- Fix 0B/44/00 error occuring during long sequential reads
- Improvments to Log Page Reporting
- Improve overlapped WCE performance
- Improved Error handling  

Model#                Criticality      File Name
-----------------    -------------  --------------------------------
HUC103014CSS600       Recommended   Hitachi_HUC103014CSS600_J516.df
HUC103030CSS600       Recommended   Hitachi_HUC103030CSS600_J516.df


-------------------------------------------------------------
16.0 Hitachi SAS 15K RPM, version K516
-------------------------------------------------------------
Fixes / Enhancments:

- Fixed rare timeout issue that can occur during a drive reset
- Fix 0B/44/00 error occuring during long sequential reads
- Improvments to Log Page Reporting
- Improve overlapped WCE performance
- Improved Error handling  

Model#               Criticality           File Name
-----------------    -----------    ----------------------------------
HUC151473CSS600    Recommended    Hitachi_HUC151473CSS600_K516.df
HUC151414CSS600    Recommended    Hitachi_HUC151414CSS600_K516.df


-------------------------------------------------------
17.0 Hitachi SAS 15K RPM, version E516
-------------------------------------------------------
Fixes / Enhancements:

- Improved Drive detection at boot up
- Corrected error handling causing a self init drive reset.
- Improve error handling during a check condition
  
Model#             Criticality      File Name
---------------    -----------      -------------------------------
HUS156030VLS600    Recommended      Hitachi_HUS156030VLS600_E516.df
HUS156045VLS600    Recommended      Hitachi_HUS156045VLS600_E516.df
HUS156060VLS600    Recommended      Hitachi_HUS156060VLS600_E516.df


------------------------------------------------------------
18.0 Pliant LB150 SSD, version D012
------------------------------------------------------------
Fixes / Enhancements:

- Improves error handling when link between host and drive occurs.
- Corrected issue causing incorrect LED behavior.  

Model#          Criticality     File Name
----------	  -------------	  ----------------------------------
LB150S         Recommended      Pliant_LB150S_D012.df


--------------------------------------------------------------------------------
19.0 Seagate (Constellation ES) SAS 3.5" 7.2K, version KSF2
--------------------------------------------------------------------------------
Fixes/Enhancements



Model #				          File Name
-------------------- ------------------------------------
ST31000425SS           Firmware version KSF2
ST32000445SS           Firmware version KSF2


--------------------------------------------------------------------------------
20.0  Western Digital (SL200M)  SAS 2.5" 10K, version D1VB**
--------------------------------------------------------------------------------
Fixes / Enhancements:
Resolves an issue that causing slower performance in RAID 5 environments
Resolves a rare issue when getting multiple start commands on warm boot
Improves performance for sequential reads with large queue depths
Improves performance for Linux DD command with transfer sizes 512K and 1MB
Improves drive error handling

Model #				           File Name
-------------------- ------------------------------------
WD3000BKHG             WD_WD3000BKHG_D1VB.df
WD6000BKHG             WD_WD6000BKHG_D1VB.df


--------------------------------------------------------------------------------
21.0  Western Digital (SL500M)  SAS 3.5" 7.2K, version D1BG**
--------------------------------------------------------------------------------

Change Description:
Resolves an issue that causing slower performance in RAID 5 environments
Resolves a rare issue when getting multiple start commands on warm boot
Improves performance for sequential reads with large queue depths
Improves performance for Linux DD command with transfer sizes 512K and 1MB
Improves drive error handling

Model #		     Criticality      File Name
-------------------- ------------   ---------------------
WD1000FYYG         Critical         WD_WD1000FYYG_D1BG.df
WD2000FYYG         Critical         WD_WD2000FYYG_D1BG.df

--------------------------------------------------------------------------------
22.0  Hitachi (Ultrastar C10K600) SAS 2.5" 10K, version A360
--------------------------------------------------------------------------------
Fixes / Enhancements:

Enhanced Drive Error Handling
Improved performance of long transfers with random commands

Model#              Criticality      File Name
----------	    -------------    ----------------------------------
HUC106030CSS600     Recommended      Hitachi_HUC106030CSS600_A360.df
HUC106060CSS600     Recommended      Hitachi_HUC106060CSS600_A360.df

--------------------------------------------------------------------------------
23.0  Seagate Constellation.2   SAS 2.5" 7.2K, version AS06
--------------------------------------------------------------------------------

Change Description:

When firmware is applied prior to a cold power cycle this firmware prevents a situation that can lead to unrecoverable drive failure during A/C power removal.
Resolves a rare condition that can cause drive to hang during power on sequence
Improvements to overall drive reliability
Improvements to background scan logging
Improved drive error handling


Model#            Criticality       File Name
----------	  -------------	  ----------------------------------
ST9500620SS       Critical        Seagate_ST9500620SS_AS06.df
ST91000640SS      Critical        Seagate_ST91000640SS_AS06.df


-----------------------------------------------------------------------
24.0 Toshiba (MBF 2 RC) 10K RPM, version DA07
-----------------------------------------------------------------------
Fixes / Enhancements:

-Improved drive motor servo related to vibratation of 220Hz and >1800Hz
-Improved performance of Sequential verify

Model#          Criticality     File Name
----------	-------------	----------------------------------
MBF2300RC       Recommended     Toshiba_MBF2300RC_DA07.df
MBF2600RC       Recommended     Toshiba_MBF2600RC_DA07.df

--------------------------------------------------------------------------------
25.0  Toshiba MK2001TRKB Series SAS 2.5" 7.2K, version DCAA
--------------------------------------------------------------------------------

Improved drive error handling
Improved long term drive reliability

Model #				             File Name
-------------------- ----------------------------------------
MK1001TRKB             Firmware version DCAA 
MK2001TRKB             Firmware version DCAA 

--------------------------------------------------------------------------------
26.0  Seagate Savvio 10K.5 SAS 2.5" 10K.5, version CS08
--------------------------------------------------------------------------------

Change Description:

Improves sequential read / write performance
Improvements to overall drive reliability
Improvements to background scan logging
Improved drive error handling


Model #		     Criticality      File Name
-------------------- -------------  -----------------------
ST9300605SS        Recommended      Seagate_ST9300605SS_CS08.df
ST9600205SS        Recommended      Seagate_ST9600205SS_CS08.df
ST9900805SS        Recommended      Seagate_ST9900805SS_CS08.df

--------------------------------------------------------------------------------
27.0  Seagate Constellation ES.2 SAS 2.5" 7.2K, version ASF9 
--------------------------------------------------------------------------------
Fixes/Enhancements

-Resolves a rare condition that can cause drive to hang during power on sequence
-Resolves a rare issue that could incorrectly incremented SMART error counter for read errors
-Resolves a rare issue that could cause to hang during format
-Resolves an issue that caused drive to connect at slower connection speeds
-Resolves an issue causing poor write performance when background scan is running
-Resolves rare issue that could cause hang during boot up with RAID controller
-Resolves issue would unexpectedly abort read command without proper reporting proper status
-Improvements to drive connectivity
-Improved drive error handling
-Improves drive long term reliablity

Model #			Criticality             File Name
-------------------- ----------------------------------------
ST91000642SS           Recommended	Firmware version ASF9

--------------------------------------------------------------------------------
28.0 Seagate (Constellation ES.2)     3.5" 7.2K,   version RSFA
--------------------------------------------------------------------------------

Resolves a rare issue that could cause to hang during format
Resolves an issue that caused drive to connect at slower connection speeds
Resolves rare issue that could cause hang during boot up with RAID controller
Resolves issue would unexpectedly abort read command without proper reporting proper status
Improvements to drive connectivity
Improved drive error handling

Model #			Criticality             File Name
-------------------- ----------------------------------------
ST33000652SS          	Recommended	 Firmware version RSFA

--------------------------------------------------------------------------------
29.0  Seagate Savvio 10K.5 SAS 2.5" 10K, version CSF8
--------------------------------------------------------------------------------
Fixes/Enhancements

-Resolves a rare issue that could incorrectly incremented SMART error counter for read errors
-Resolves a rare issue that could cause to hang during format
-Resolves an issue that caused drive to connect at slower connection speeds
-Resolves an issue causing poor write performance when background scan is running
-Resolves rare issue that could cause hang during boot up with RAID controller
-Resolves issue would unexpectedly abort read command without proper reporting proper status
-Improvements to drive connectivity
-Improved drive error handling
-Improves drive long term reliablity


Model #			Criticality            File Name
-------------------- ----------------------------------------
ST9900605SS           Recommended	 Firmware version CSF8

--------------------------------------------------------------------------------
30.0  Seagate Savvio 15K.3 SAS 2.5" 15K, version YSF9
--------------------------------------------------------------------------------

Resolves a rare issue that could incorrectly incremented SMART error counter for read errors
Resolves a rare issue that could cause to hang during format
Resolves an issue that caused drive to connect at slower connection speeds
Resolves an issue causing poor write performance when background scan is running
Resolves rare issue that could cause hang during boot up with RAID controller
Resolves issue would unexpectedly abort read command without proper reporting proper status
Improvements to drive connectivity
Improved drive error handling
Improves drive long term reliablity

Model #		     Criticality             File Name
-------------------- ----------------------------------------
ST9300453SS          Recommended	Firmware version YSF9

--------------------------------------------------------------------------------
31.0  Seagate Savvio 15K.3 SAS 2.5" 15K, version YS09 
--------------------------------------------------------------------------------

Change Description:

-Resolved an rare issue with multiple start commands could trigger wrong sense code
-Improved drive error handling
-Improved drive error logging
-Improved drive long term reliablitiy
-Enable Persistent Reservation

Model #		     Criticality    File Name
-------------------- -----------  -----------------------
ST9146853SS        Recommended    Seagate_ST9146853SS_YS09.df
ST9300653SS        Recommended    Seagate_ST9300653SS_YS09.df

--------------------------------------------------------------------------------
32.0  Seagate Constellation ES.2 SAS 3.5" 7.2K, version RS11
--------------------------------------------------------------------------------
Change Description:

-Resolves an issue that can drive to hang during powering on
-Resolves an issue where drive can reject command after link reset
-Improved drive error handling
-Improved Linear Vibration robustness

Model#              Criticality     File Name
---------------     -----------	  ----------------------------
ST32000645SS	  Recommended      Seagate_ST32000645SS_RS11.df
ST33000650SS      Recommended      Seagate_ST33000650SS_RS11.df 

--------------------------------------------------------------------------------
**33.0  Seagate Constellation ES SAS 3.5" 7.2K, version PS07 
--------------------------------------------------------------------------------
Change Description:

Resolved an rare issue with multiple start commands could trigger wrong sense code
Improved drive error handling
Improved drive error logging
Improved drive long term reliablitiy
Enable Persistent Reservation

Model #		     Criticality     File Name
-------------------- ------------  -----------------------
ST500NM0001        Recommended     Seagate_ST500NM0001_PS07.df
ST1000NM0001       Recommended     Seagate_ST1000NM0001_PS07.df
ST2000NM0001       Recommended     Seagate_ST2000NM0001_PS07.df

--------------------------------------------------------------------------------
34.0 Toshiba MD2001GRZB Series SAS 2.5" SSD, version A006
--------------------------------------------------------------------------------
Change Description:

Improved error handling

Model #		     Criticality     File Name
-------------------- ------------  -----------------------
MD2001GRZB         Recommended     Toshiba_MD2001GRZB_A006.df
MD4001GRZB         Recommended     Toshiba_MD4001GRZB_A006.df


--------------------------------------------------------------------------------
35.0 Western Digital (SL300M)	      2.5" 10K	   version D1S4
--------------------------------------------------------------------------------

Change Description:

Improved sequential write performance under RAID 5 configurations
Improved write through performance
Improved drive error handling
Improved drive reliability


Model #		     Criticality     File Name
-------------------- ------------  -----------------------
WD3001BKHG           Recommended   WD_WD3001BKHG_D1S4.df
WD6001BKHG           Recommended   WD_WD6001BKHG_D1S4.df
WD9001BKHG           Recommended   WD_WD9001BKHG_D1S4.df

--------------------------------------------------------------------------------
36.0 Hitachi Ultrastar   7K3000	      3.5" 7.2K	   version M2D4
--------------------------------------------------------------------------------

Change Description:

Fixes 04/44 issues in field

Model #		     Criticality     File Name
-------------------- ------------  -----------------------
HUS723020ALS640	     Recommended   Hitachi_HUS723020ALS640_M2D4.df
HUS723030ALS640	     Recommended   Hitachi_HUS723030ALS640_M2D4.df


--------------------------------------------------------------------------------
37.0 Hitachi Ultrastar C10K600        2.5" 10K     version N2B4
--------------------------------------------------------------------------------


Model #		    Criticality 	File Name
---------------------------------------------------------
HUC109030CSS600	    Recommended	        Firmware version N2B4 (pre-load) 
HUC109060CSS600	    Recommended  	Firmware version N2B4 (pre-load) 
HUC109090CSS600	    Recommended		Firmware version N2B4 (pre-load) 

-------------------------------------------------------------------------------
38.0 Toshiba AL12SX		      2.5" 15k,	   version DB05
--------------------------------------------------------------------------------
Fixes/Enhancements

-Resolve issue with Dell Diagnostic Utility that incorrectly caused Read Buffer error
-Resolved connectivity issue that could occur on power cycle

Model #		Criticality   		 File Name
-----------------------------------------------------------
MK1401GRRB	Recommended	      	Firmware version DB05  
MK3001GRRB	Recommended		Firmware version DB05


--------------------------------------------------------------------------------
39.0 Toshiba AL12SE	      2.5", 10k,   version DA0B
--------------------------------------------------------------------------------
Fixes/Enhancements

-Resolve issue with Dell Diagnostic Utility that incorrectly caused Read Buffer error
-Resolved connectivity issue that could occur on power cycle

Model #			Criticality	     File Name
--------------------------------------------------------
MBF2300RC		Recommended	Firmware version DA0B  
MBF2600RC		Recommended	Firmware version DA0B


Model #			Criticality	     File Name
--------------------------------------------------------
MBF2300RC		Recommended	Firmware version DA0B (pre-load) 
MBF2600RC		Recommended	Firmware version DA0B


--------------------------------------------------------------------------------
40.0 Seagate (ST*00MM0006)	      2.5" 10k	   version LS06**
--------------------------------------------------------------------------------
Fixes/Enhancements
Initial Release

Model #			Criticality	     File Name
--------------------------------------------------------
ST300MM0006		Recommended	Seagate_ST300MM0006_LS06.df
ST600MM0006		Recommended	Seagate_ST600MM0006_LS06.df
ST900MM0006		Recommended	Seagate_ST900MM0006_LS06.df

--------------------------------------------------------------------------------
41.0 Sandisk Everest		      2.5"	   version D313**
--------------------------------------------------------------------------------
Fixes/Enhancements
Initial Release

Model #			Criticality	     File Name
--------------------------------------------------------
LB 206M 		Recommended	Version D313 (pre-load)
LB 406M 		Recommended	Version D313 (pre-load)

--------------------------------------------------------------------------------
42.0 WD Verdi			      3.5" 7.2K	   version D1R2**
--------------------------------------------------------------------------------
Fixes/Enhancements
Initial Release

Model #			Criticality	     File Name
--------------------------------------------------------
WD1001FYYG 		Recommended	Version D1R2 (pre-load)
WD2001FYYG		Recommended	Version D1R2 (pre-load)
WD3001FYYG		Recommended	Version D1R2 (pre-load)
WD4001FYYG		Recommended	Version D1R2 (pre-load)